Set up your Trekz Titanium

Step 1. Charge

Charge the headphones with the included micro-USB charging cable. The micro-USB charging port is located on the right side of the headphones (as worn) and enclosed by a small protective hinged cover. The hinged cover can be lifted by using a fingernail. When the hinged cover is lifted, the Micro-USB charging port is revealed. The LED indicator will turn blue when charging is complete.

Step 2. Pair

While off, press and hold the power button for 5 seconds to enter pairing mode. The LED indicator will flash blue and red repeatedly while in discovery.

Step 3. Connect

Enable the Bluetooth® settings on your device and select “Trekz Titanium by AfterShokz”. The LED indicator will turn blue once connected.

How to wear

Begin by holding the headphones horizontally, with the transducer side facing up, closest to your body. Lift the headphones over your head, so the back of the wraparound headband sets in place at the base of the head, and the transducers rest on your cheekbones in front of your ears (not nested inside or covering your ears).

Multifunction Button Functions and Prompts

(The multifunction button is a triangle button located on the outside of the left transducer)

**Play/pause music:**

Click the multifunction button once.

One beep.

**Skip to next song:**

Double-click the multifunction button while music is playing.

One beep.

**Answer/end call:**

Click the multifunction button once.

One beep.

**Answer call waiting and put the current caller on hold:**

Click the multifunction button once to switch between callers.

One beep.

**Answer call waiting and hang up on current caller:**

Press and hold the multifunction button for 2 seconds.

One beep.

**Reject a call:**

Press and hold the multifunction button for 2 seconds.

Two beeps.

**Voice dial:**

Press and hold the multifunction button for 2 seconds.

“Voice dial”.

**Redial last number:**

Double-click the multifunction button.

“Last number redial”.

Volume/Power Button Functions and Prompts

(The volume/power buttons are located on the underside of the right arm of the headphone. The volume up button has a raised dot on it. The volume up button also acts as the power button. The volume down button is the button next to the volume up and power button.)

**Power on/off**

Press and hold the power button for 2 seconds

Four beeps and “welcome to Trekz Titanium”

**Mute**

Press and hold both for 2 seconds while on a call

“Mute on” or “mute off”

**Change EQ setting**

Press and hold both for 2 seconds while music is playing

“Equalization changed”

**Check battery status**

Click the volume up or down while music is paused

“Battery high, medium, low, or charge me”

**Adjust volume**

Click the volume up or down button to adjust volume

One beep

Specifications

**Part number**

AS600

**Speaker type**

Bone conduction transducer

**Frequency response**

20Hz~20KHz

**Sensitivity**

100 ± 3dB

**Microphone**

-40dB ± 3dB

**Bluetooth version**

Bluetooth® v4.1

**Compatible profiles**

A2DP, AVRCP, HSP, HFP

**Wireless range**

33 ft (10m)

**Battery**

Rechargeable lithium ion

**Continuous play**

6 hours

**Standby time**

10 days

**Charge time**

1.5 hours

**Weight**

1.27 oz (36g)

**Warranty**

2 years

Muiltipoint pairing

Step 1. Enter pairing mode

Step 2. Press Multifunction button + volume up/power button for 2 seconds (Audrey SaysTM“multipoint enabled”)

Step 3. Pair first device (Audrey SaysTM “Connected”)

Step 4. Shut down

Step 5.  Re-enter pairing mode

Step 6.  Pair second device (Audrey SaysTM “second device connected”)

Step 7.Turn the device off, then power back on

LED indicator

**Solid red:** Charging

**Solid blue:** Charging complete

**Flashes red and blue:** Pairing mode

**Flashes blue:** Incoming call

**Flashing red every 2 minutes:** Low battery

How to reset your headphones

Enter pairing mode, then press and hold the multifunction button, and both volume buttons for 3 seconds.

To validate your 2-year warranty, register your product at

http://bit.ly/RegisterMyTrekz

Only purchases from authorized resellers are supported by our warranty policy.

Optional Accessories

Fitband

Silicon rubber bands provide adjustability to accommodate smaller head sizes.

Step 1. Slide Fitband over the right transducer and along the right arm to rest over the charging port.

Step 2. Slide the second Fitband over the left transducer and along the left arm to align evenly with the right arm.

Step 3. Rotate the Fitbands around the arms until the desired fit is achieved.

Earplugs

Use with headphones in environments where it is safe to block out ambient noise, such as on an airplane or train.

Step 1. Roll earplugs firmly between fingers and place in ears.

Step 2. To adjust EQ settings to reduce or enhance bass while wearing earplugs, press and hold volume up and down buttons simultaneously.

Step 3. Switch EQ to normal condition when you take out the earplug.